Window handle F2304  56 Denver
Lever version in color 56
by KARCHER DESIGN

Secure fixing oval back plate
with M5 threaded screws
rotational operation in 4 positions
3/8” (10 mm) lugs and
nylon floating bearing,
5/16” (7 mm) spindle,
length: 1 3/8” (35 mm)
screw fixing centre 1 11/16” (43 mm)

Special options
EAR 400 (key operated)
For burglary-resistant windows,
cylinder lock operation

Finish: satin/polished chrome (finish code 56)
Karcher article no.:
F2304 56	window handle Denver

Dimensional detail:

Window Handle			Lockable window handle 

5 ¼“ (134mm)

2 3/16“ (55mm)

15/16“(24mm)

13/16“ (20mm)

½“ (12,5mm)

2 ½“ (65mm)

1 „ (25mm)

1 ¼“ (32mm)

3 7/8“ (99mm)