Pull handle ES 2
by KARCHER DESIGN

Oval Shape, massive stainless steel
2 fixing points

Please note: Karcher Design products are designed and measured in metric. The inch measurements are close approximations to the actual metric dimensions 

Fixing centre: 11 13/6” (300 mm)
Overall: 13 ¾” (350 mm)
Handle diameter: 1” (25 mm)
Fixing with M8
single bolt through fixing
or back to back pair fixing
For timber, metal, PVC or glass door

Finish: satin stainless steel (finish code 71)

Karcher article no.:
ES2-300 
ES2G-300 

Bolt fixings:
EZ1060 back to back fixing as pair for timber, metal or PVC door
EZ1063 secret face fixing for timber doors
EZ1064 secret face fixing for frame/PVC doors
EZ1065 bolt through fixing for timber or frame door with cover caps on the opposite side
EZ1066 bolt through fixing without cover caps (single fixing)

Dimensional detail:

2 ½“
63mm

2 3/8“ (60mm)

ES2G 300

55º

2 15/16“
(75mm)

1“ (25mm)

11 13/16“
(300mm)

1“ (25mm)

2 15/16“
(75mm)

11 13/16“ 
(300mm)