Pull handle ES4P 350
by KARCHER DESIGN

T-Shape stainless steel 
2 fixing points 
Satin stainless steel 
Overall: 13 ¾” or 19 11/16” (350 mm or 500 mm)
Handle diameter: 1” (25 mm)
Fixing with M8 
Fixing as pair for glass
Drilling diameter in the glass ½” or 7/8” (13 mm or 22 mm)

Finish: satin stainless steel
Karcher article no.:
ES4P-350 71 straight  (overall 13 ¾” (350 mm), fixing centre 5 7/8” (150 mm))
ES4P-500 71 straight  (overall 19 11/16” (500 mm), fixing centre 11 13/16” (300 mm))

Fixing possibilities:
As pair for glass
Fixing included

Dimensional detail:

13 ¾“ or 19 11/16“
(350mm o.500mm)

1“ (25mm)

 3 5/16“ (84mm)

Please note: Karcher Design products are designed and measured in metric. The inch measurements are close approximations to the actual metric dimensions