Backplate RLE32 Babylon for Multi point lock
by KARCHER DESIGN

Lever handle on plate 10 ¼” x 2 1/16” (260 x 52 mm),
with dual fixing and nylon floating bearing,
unsprung, with ER32 Babylon,
M4 bolt through fixing,
5/16” (8mm) offset drilled spindle,
standard door thickness: 1 ¾” (45mm)

Options: Backplates without cylinder and without Multipoint lock
ENT: Backplate for Entrance Profile Cylinder Multipoint Lock
PAS : Backplate for Passage Multi Point Lock
HIHP: Backplate Half Inactive Half passage Multipoint
DUM: Backplate for Full Inactive Multipoint Lock     
PAT: Backplate Patio Multi Point

Finish Plate: satin stainless steel (finish code 71)
Finish handle: Polished/Satin stainless steel (finish code 73)
Karcher article no.:
RLE32 ENT 73
RLE32 PAS 73
RLE32 HIHP 73
RLE32 DUM 73
RLE32 PAT 73

5 1/8“ (130mm)

2 3/16“ (56mm)

15/16“  X 11/16“
(24 X 17mm)

Please note: Karcher Design products are designed and measured in metric. The inch measurements are close approximations to the actual metric dimensions 

2 1/16”
(52mm)

3/8”
(10mm)

10 1/4” 
(260mm)

7/8” (22mm)

3 15/16” (100mm)

3 5/8” (92mm)

7/8” 22

Dimensional detail: